**F-TYPE SVR 2017 MY TECHNICAL DATA**

|  |  |  |
| --- | --- | --- |
|  | **F-TYPE SVR Coupé** | **F-TYPE SVR Convertible** |
| **ENGINE & TRANSMISSION** |  | |
| Engine capacity (cc) | 5,000 | |
| Cylinders | V8 Supercharged | |
| Valves per cylinder | 4; DOHC | |
| Bore/ stroke (mm) | 92.5/ 93.0 | |
| Compression ratio | 9.5:1 | |
| Fuel injection | 150bar direct injection | |
| Power PS (kW) | 575 (423) @ 6,500rpm | |
| Torque Nm (lb ft) | 700 (516) @ 3,500-5,000rpm | |
| Transmission | 8-speed Quickshift | |
| Gear ratios (:1) |  | |
| 1st | 4.714 | |
| 2nd | 3.143 | |
| 3rd | 2.106 | |
| 4th | 1.667 | |
| 5th | 1.285 | |
| 6th | 1.000 | |
| 7th | 0.839 | |
| 8th | 0.667 | |
| Reverse | 3.317 | |
| Final Drive ratio | 2.56 | |
| **CHASSIS** |  | |
| Front suspension | Double wishbone | |
| Rear suspension | Double wishbone | |
| Front brakes | Twin-piston sliding caliper; 380mm ventilated discs | |
| Rear brakes | Single-piston sliding caliper; 376mm ventilated discs | |
| Front tyres | 265/35/ZR20 Pirelli P Zero | |
| Rear tyres | 305/30/ZR20 Pirelli P Zero | |
| Steering | Rack-and-pinion; electromechanical | |
| **DIMENSIONS** |  |  |
| Length (mm) | 4,475 | 4,475 |
| Width inc./ excl. mirrors (mm) | 2,042/ 1,923 | 2,042/ 1,923 |
| Height (mm) | 1,311 | 1,308 |
| Wheelbase (mm) | 2,622 | 2,622 |
| Track front/ rear (mm) | 1,585/ 1,611 | 1,585/ 1,611 |
| Weight (kg) | From 1,705 | From 1,720 |
| Boot volume (litres) | 310/ 408 with/ without parcel tray | 206.7 |
| Fuel tank (useable) litres | 70 | 70 |
| **PERFORMANCE & FUEL ECONOMY** |  |  |
| 0-60mph (sec) | 3.5 | 3.5 |
| 0-100km/h (sec) | 3.7 | 3.7 |
| Top speed mph (km/h) | 200 (322) | 195 (314) |
| Fuel consumption mpg (litres/100km) EU combined | 25.0 (11.3) | 25.0 (11.3) |
| CO2 emissions (g/km) EU combined | 269 | 269 |

Manufacturer’s figures; correct at time of going to press